TRE C – T24 SYSTEM
VOCI DI CAPITOLATO
TECHNICAL SPECIFICATIONS

Voci di capitolato
I pannelli del controsoffitto T24 SYSTEM prodotti da TRE C saranno realizzati in acciaio zincato a caldo preverniciato spessore 0.6mm. La finitura dei pannelli sarà bianco luminoso, ref. W722.
Ogni pannello sarà completamente ispezionabile e avrà superficie microforata. La foratura avrà fori diametro 1.5mm sfalsati a 45° con rapporto V/P 22%. I pannelli avranno uno scuretto non forato da 10mm sui quattro lati. Verrà applicato un velo acustico nero sul lato interno per migliorare le prestazioni acustiche del controsoffitto.
Il modulo unitario misurerà 600x600 mm (575x575 mm effettivi), con appoggio complanare alla struttura “T”, tipo R0.
I pannelli risponderanno alla classe di reazione al fuoco Euroclasse A2 (D.M. del 15 Marzo 2005); manterranno stabilità dimensionale anche in situazioni ambientali estreme e potranno essere installati in ambienti con elevati tassi d’umidità relativa e notevoli sbalzi termici. Per l’impiego in esterni si consiglia di contattare l’ufficio tecnico TRE C.
Ciascun pannello sarà installato ad appoggio su specifica struttura di sostegno a vista Sistema T24 prodotta da TRE C composta da profilo portante a “T” tipo TRE C W_T24_PORT_38x24, profili intermedi da 1200 e 600 mm tipo W_T24_INT_38x24x1200 e W_T24_INT_38x24x600 di colore bianco.
I profili della struttura verranno collegati al solaio mediante pendinatura W_PEND_D4_500 in filo di metallico D=4mm L=500mm e molla con pendino a "C" fisso W_T24_GANC-MOLL.
Lungo il perimetro il controsoffitto sarà rifinito con apposito profilo perimetrale in acciaio W_PL_20x40 colore bianco, corredato da molle antisollevamento in acciaio armonico TRE C W_MOLL_40x20.

Specifications
The T24 SYSTEM ceiling panels manufactured by TRE C will be made of hot-dip galvanized pre-painted steel, 0.6mm thick. The panels will have a bright white finish, ref. W722.
Each panel will be fully inspectable and have a micro-perforated surface. The perforation will have 1.5mm diameter holes offset at 45° with a open ratio of 22%.
The panels will have a 10mm non-perforated border on all four sides. A black acoustic veil will be applied to the inner side to improve the ceiling's acoustic performance.
The unit module will measure 600x600 mm (575x575 mm effective), with a co-planar support on the "T" structure, type R0.
The panels will meet the Euroclass A2 fire reaction class (D.M. of 15 March 2005); they will maintain dimensional stability even in extreme environmental conditions and can be installed in environments with high relative humidity and significant temperature variations. For outdoor use, please contact the TRE C technical office.
Each panel will be installed on a specific visible support structure, T24 System manufactured by TRE C, consisting of a "T" shaped carrying profile, type TRE C W_T24_PORT_38x24, intermediate profiles of 1200 and 600 mm, type W_T24_INT_38x24x1200 and W_T24_INT_38x24x600, in white. The structure profiles will be connected to the ceiling using W_PEND_D4_500 suspension wires, D=4mm L=500mm, and a spring with a fixed "C" hook, W_T24_GANC-MOLL. Along the perimeter, the ceiling will be finished with a special white steel perimeter profile, W_PL_20x40, equipped with TRE C W_MOLL_40x20 harmonic steel anti-lift springs.
